1. .Read request from L1 data.
   1. Hit
      1. Modified
         1. MESI - Stays M
         2. Pass data to L1 Data
      2. Exclusive
         1. MESI - Stays E
            1. Pass data to L1 Data
      3. Shared
         1. MESI – Stays S
            1. Pass data to L1 Data
      4. Invalid
         1. HIT
            1. MESI – S

Get data from shared bus

* + - 1. MISS (HIT')
         1. MESI – E

Get data from shared bus as RFO

* 1. Miss
     1. HIT from other processor
        1. MESI – E
        2. Read data from shared bus
        3. Place in L2
        4. Pass to L1 Data.
     2. MISS from other processor
        1. MESI - E
        2. Read data from shared bus as RFO
        3. Place in L2

1. Write request from L1 data
   1. Hit
      1. Modified
         1. MESI – Stays M
         2. Write to L2 cache
      2. Exclusive
         1. MESI – M
         2. Write to L2 cache
      3. Shared
         1. MESI – M
         2. Read from shared bus with RFO or Invalidate
         3. Write to L2 cache
      4. Invalid
         1. MESI – M
         2. Read from shared bus with RFO
         3. Write to L2 cache
   2. Miss
      1. Read from shared bus with RFO (done for inclusivity?)
2. Read request from L1 instruction
   1. Hit
      1. Modified
         1. Shouldn’t happen because it is an instruction
      2. Exclusive
         1. MESI - Stays E
            1. Pass data to L1 Instruction
      3. Shared
         1. MESI – Stays S
            1. Pass data to L1 Instruction
      4. Invalid
         1. HIT
            1. MESI – S

Get data from shared bus

* + - 1. MISS (HIT')
         1. MESI – E

Get data from shared bus as RFO

* 1. Miss
     1. HIT from other processor
        1. MESI – E
        2. Read data from shared bus
        3. Place in L2
        4. Pass to L1 Data.
     2. MISS from other processor
        1. MESI - E
        2. Read data from shared bus as RFO
        3. Place in L2

1. Snooped invalidate command (Another processor is modifying the data)
   1. Modified
      1. This should not happen due to MESI protocol
   2. Exclusive
      1. MESI
         1. If RFO: Invalidate
         2. If Read: Shared
   3. Shared
      1. MESI - I
   4. Invalid
      1. MESI – Stays I
2. Snooped read request (another processor is trying to read)
   1. HIT/HITM
      1. Modified
         1. MESI – S
         2. Write back to shared bus
      2. Exclusive
         1. MESI – S
      3. Shared
         1. MESI – Stay S
      4. Invalid
         1. Do nothing
   2. MISS
      1. Put miss
         1. Do nothing
3. Snooped write request (another processor is trying to write)
   1. HIT/HITM
      1. Modified
         1. This will not happen due to MESI protocol.
      2. Exclusive
         1. Will never happen due to MESI protocol. If another processor has it and has modified it, we will definitely be in the Invalid state.
      3. Shared
         1. This will not happen due to MESI protocol.
      4. Invalid
         1. Do nothing
   2. MISS
      1. Do nothing
4. Snooped read with intent to modify
   1. HIT/HITM
      1. Modified
         1. MESI – I
         2. Write back to shared bus
      2. Exclusive
         1. MESI – I
      3. Shared
         1. MESI – I
      4. Invalid
         1. Do nothing
   2. MISS
      1. Do nothing
5. Clear and reset all
   1. Invalidate all memory locations. It is not necessary to clear the memory locations.
6. Print contents and state of each valid line
   1. Print contents and states of all(only) valid lines

Notes:

1. Read For Ownership (RFO) – Do a memory read but indicate to snooping processors on FSB our intent to write that memory location (slide 62)
2. Invalidate – “Invalidate your copy and I have the only valid one now.” Address only transaction (i.e.: Puts address on the FSB but doesn’t request data from memory)
3. IMPORTANT: Slide 68
   1. Constraints are met
   2. If miss in both L1 and L2, line is placed in both caches
      1. If a dirty line is evicted from L1 it will be held in L2 (IP).
      2. If a dirty line is evicted from L2 it must also be evicted from L1 (IP)
   3. Miss to L1 and hit to L2
      1. Due to a line being evicted from L1 where it is written back to L2 (IP)
   4. On a snoop hit to L2, L2 instructs L1 to invalidate the line in its cache
      1. Minimize invalidates by keeping single bit/line in L2 to indicate in L1
   5. Relaxed constraints
      1. L2 line size = C \* L1 line size (where C >= 1)
      2. Need additional inclusion bits if C > 1
      3. Associativity L2 / L2 line size >= Associativity L1 / L1 line size
4. IMPORTANT: Slide 65
   1. Has a MESI FSM that was used by PowerPC that incorporates the MESI protocol and the required functions for all cases into the one FSM. FSM and notes found below.

